# AI on the Edge Device - Webinstaller

# AI-on-the-edge-device

## Webinstaller and Console

This page provides the Webinstaller and a live USB Console to your AI-on-the-edge-device.
For further information about AI-on-the-edge-device please go to https://github.com/jomjol/AI-on-the-edge-device.

Notes:

- For the installation, make sure to switch the ESP32 to Bootloader mode!
- After the installation, a manual reset might be required!
- Please note that not all webbrowsers and operating systems support the needed access to USB!
- Check the documentation for additional information.
- The SD-Card still must be setup separately. This can be done manually or using the new Remote Setup. See the documentation for further instructions!

Installer and Console powered by ESP Web Tools